Architecture:                    aarch64
CPU op-mode(s):                  32-bit, 64-bit
Byte Order:                      Little Endian
CPU(s):                          256
On-line CPU(s) list:             0-255
Thread(s) per core:              1
Core(s) per socket:              128
Socket(s):                       2
NUMA node(s):                    2
Vendor ID:                       ARM
Model:                           1
Model name:                      Neoverse-N1
Stepping:                        r3p1
Frequency boost:                 disabled
CPU max MHz:                     3000.0000
CPU min MHz:                     1000.0000
BogoMIPS:                        50.00
L1d cache:                       16 MiB
L1i cache:                       16 MiB
L2 cache:                        256 MiB
NUMA node0 CPU(s):               0-127
NUMA node1 CPU(s):               128-255
Vulnerability Itlb multihit:     Not affected
Vulnerability L1tf:              Not affected
Vulnerability Mds:               Not affected
Vulnerability Meltdown:          Not affected
Vulnerability Spec store bypass: Mitigation; Speculative Store Bypass disabled via prctl
Vulnerability Spectre v1:        Mitigation; __user pointer sanitization
Vulnerability Spectre v2:        Not affected
Vulnerability Srbds:             Not affected
Vulnerability Tsx async abort:   Not affected
Flags:                           fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp cpuid asimdrdm lrcpc dcpop asimddp ssbs
