Architecture:                    x86_64
CPU op-mode(s):                  32-bit, 64-bit
Address sizes:                   39 bits physical, 48 bits virtual
Byte Order:                      Little Endian
CPU(s):                          6
On-line CPU(s) list:             0-5
Vendor ID:                       GenuineIntel
Model name:                      Intel(R) Core(TM) i5-8400 CPU @ 2.80GHz
CPU family:                      6
Model:                           158
Thread(s) per core:              1
Core(s) per socket:              6
Socket(s):                       1
Stepping:                        10
CPU max MHz:                     4000.0000
CPU min MHz:                     800.0000
BogoMIPS:                        5602.18
Flags:                           fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush dts acpi mmx fxsr sse sse2 ss ht tm pbe syscall nx pdpe1gb rdtscp lm constant_tsc art arch_perfmon pebs bts rep_good nopl xtopology nonstop_tsc cpuid aperfmperf pni pclmulqdq dtes64 monitor ds_cpl vmx est tm2 ssse3 sdbg fma cx16 xtpr pdcm pcid sse4_1 sse4_2 x2apic movbe popcnt tsc_deadline_timer aes xsave avx f16c rdrand lahf_lm abm 3dnowprefetch cpuid_fault epb invpcid_single pti ibrs ibpb stibp tpr_shadow vnmi flexpriority ept vpid ept_ad fsgsbase tsc_adjust bmi1 avx2 smep bmi2 erms invpcid mpx rdseed adx smap clflushopt intel_pt xsaveopt xsavec xgetbv1 xsaves dtherm ida arat pln pts hwp hwp_notify hwp_act_window hwp_epp
Virtualization:                  VT-x
L1d cache:                       192 KiB (6 instances)
L1i cache:                       192 KiB (6 instances)
L2 cache:                        1.5 MiB (6 instances)
L3 cache:                        9 MiB (1 instance)
NUMA node(s):                    1
NUMA node0 CPU(s):               0-5
Vulnerability Itlb multihit:     KVM: Mitigation: VMX disabled
Vulnerability L1tf:              Mitigation; PTE Inversion; VMX conditional cache flushes, SMT disabled
Vulnerability Mds:               Vulnerable: Clear CPU buffers attempted, no microcode; SMT disabled
Vulnerability Meltdown:          Mitigation; PTI
Vulnerability Spec store bypass: Vulnerable
Vulnerability Spectre v1:        Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnerability Spectre v2:        Mitigation; Full generic retpoline, IBPB conditional, IBRS_FW, STIBP disabled, RSB filling
Vulnerability Srbds:             Vulnerable: No microcode
Vulnerability Tsx async abort:   Not affected
